

L

h



Wall – no slip

Outlet - pressure

Inlet - velocity

1 m