



L

h

Wall – no slip

Outlet - pressure

Inlet - pressure

1 m